-------------------------------------------------------------------------------
                             C Interface to LAPACK
                                   README
-------------------------------------------------------------------------------
Introduction
-------------------------------------------------------------------------------

This library is a part of reference implementation for the C interface to
LAPACK project according to the specifications described at the forum for 
the Intel(R) Math Kernel Library (Intel(R) MKL):
http://software.intel.com/en-us/forums/showthread.php?t=61234

This implementation provides a native C interface to LAPACK routines available
at www.netlib.org/lapack to facilitate usage of LAPACK functionality 
for C programmers.
This implementation introduces:
- row-major and column-major matrix layout controlled by the first function 
  parameter;
- an implementation with working arrays (middle-level interface) as well as 
  without working arrays (high-level interface);
- input scalars passed by value;
- error code as a return value instead of the INFO parameter.

This implementation supports both the ILP64 and LP64 programming models, 
and different complex type styles: structure, C99.

This implementation includes interfaces for the LAPACK-3.2.1 Driver and 
Computational routines only.

-------------------------------------------------------------------------------
Product Directories
-------------------------------------------------------------------------------

The installation directory of this package has the following structure:

src                - C interface source files
utils              - C interface auxiliary files
include            - header files for C interface

-------------------------------------------------------------------------------
Installation
-------------------------------------------------------------------------------

The reference code for the C interface to LAPACK is built similarly to the
Basic Linear Algebra Subprograms (BLAS) and LAPACK. The build system produces 
a static binary lapacke.a.

You need to provide a make.inc file in the top directory that defines the
compiler, compiler flags, names for binaries to be created/linked to. You may
choose the appropriate LP64/ILP64 model, convenient complex type style, 
LAPACKE name pattern, and/or redefine system malloc/free in make.inc. Several
examples of make.inc are provided.

After setting up the make.inc, you can build C interface to LAPACK by typing

make lapacke

-------------------------------------------------------------------------------
Handling Complex Types
-------------------------------------------------------------------------------

The interface uses complex types lapack_complex_float/lapack_complex_double.
You have several options to define them:

1) C99 complex types (default):

#define lapack_complex_float    float _Complex
#define lapack_complex_double   double _Complex

2) C structure option (set by enabling in the configuration file):
-DHAVE_LAPACK_CONFIG_H  -DLAPACK_COMPLEX_STRUCTURE

typedef struct { float real, imag; } _lapack_complex_float;
typedef struct { double real, imag; } _lapack_complex_double;
#define lapack_complex_float  _lapack_complex_float
#define lapack_complex_double _lapack_complex_double

3) C++ complex types (set by enabling in the configuration file): 
-DHAVE_LAPACK_CONFIG_H -DLAPACK_COMPLEX_CPP

#define lapack_complex_float std::complex<float>
#define lapack_complex_double std::complex<double>

You have to compile the interface with C++ compiler with C++ types.

4) Custom complex types:
-DLAPACK_COMPLEX_CUSTOM

To use custom complex types, you need to:
- Define lapack_complex_float/lapack_complex_double types on your own. 
- Optionally define lapack_make_complex_float/lapack_make_complex_double_real
  functions if you want to build the testing suite supplied. Use these 
  functions for the testing system. Their purpose is to make a complex value of
  a real part re, imaginary part im. The prototypes are as follows:

   lapack_complex_float lapack_make_complex_float( float re, float im );
   lapack_complex_double lapack_make_complex_double( double re, double im );

-------------------------------------------------------------------------------
Choosing ILP64 Data Model
-------------------------------------------------------------------------------
To choose ILP64 data model (set by enabling in the configuration file), use the 
following options:

-DHAVE_LAPACK_CONFIG_H  -DLAPACK_ILP64

-------------------------------------------------------------------------------
Using Predicate Functions
-------------------------------------------------------------------------------

The functions 

lapacke_?gees/lapacke_?gees_work
lapacke_?geesx/lapacke_?geesx_work
lapacke_?geev/lapacke_?geev_work
lapacke_?geevx/lapacke_?geevx_work

require the pointer to a predicate function as an argument of a predefined type
such as:

typedef lapack_logical (*LAPACK_S_SELECT2) ( const float*, const float* );

The purpose and format of these predicate functions are described in the LAPACK
documentation. This interface passes the pointer to the corresponding LAPACK
routine as it is.

Be cautious with return values of the logical type if you link against LAPACK
compiled with Fortran compiler. Whereas all non-zero values are treated as TRUE
generally, some Fortran compilers may rely on a certain TRUE value, so you will
have to use the same TRUE value in the predicate function to be consistent with
LAPACK implementation.

-------------------------------------------------------------------------------
Implementation Details
-------------------------------------------------------------------------------

The current C interface implementation consists of wrappers to LAPACK routines.
The row-major matrices are transposed on entry to and on exit from the LAPACK
routine, if needed. Top-level interfaces additionally allocate/deallocate
working space on entry to and on exit from the LAPACK routine.

Because of possible additional transpositions, a routine called with 
this interface may require more memory space and run slower than the 
corresponding LAPACK routine.

-------------------------------------------------------------------------------
Disclaimer and Legal Information
-------------------------------------------------------------------------------

INFORMATION IN THIS DOCUMENT IS PROVIDED IN CONNECTION WITH INTEL(R)
PRODUCTS. NO LICENSE, EXPRESS OR IMPLIED, BY ESTOPPEL OR OTHERWISE, TO
ANY INTELLECTUAL PROPERTY RIGHTS IS GRANTED BY THIS DOCUMENT.  EXCEPT
AS PROVIDED IN INTEL'S TERMS AND CONDITIONS OF SALE FOR SUCH PRODUCTS,
INTEL ASSUMES NO LIABILITY WHATSOEVER, AND INTEL DISCLAIMS ANY EXPRESS
OR IMPLIED WARRANTY, RELATING TO SALE AND/OR USE OF INTEL PRODUCTS
INCLUDING LIABILITY OR WARRANTIES RELATING TO FITNESS FOR A PARTICULAR
PURPOSE, MERCHANTABILITY, OR INFRINGEMENT OF ANY PATENT, COPYRIGHT OR
OTHER INTELLECTUAL PROPERTY RIGHT.  UNLESS OTHERWISE AGREED IN WRITING
BY INTEL, THE INTEL PRODUCTS ARE NOT DESIGNED NOR INTENDED FOR ANY
APPLICATION IN WHICH THE FAILURE OF THE INTEL PRODUCT COULD CREATE A
SITUATION WHERE PERSONAL INJURY OR DEATH MAY OCCUR.

Intel may make changes to specifications and product descriptions at
any time, without notice. Designers must not rely on the absence or
characteristics of any features or instructions marked "reserved" or
"undefined." Intel reserves these for future definition and shall have
no responsibility whatsoever for conflicts or incompatibilities
arising from future changes to them. The information here is subject
to change without notice. Do not finalize a design with this
information.

The products described in this document may contain design defects or
errors known as errata which may cause the product to deviate from
published specifications. Current characterized errata are available
on request.

Contact your local Intel sales office or your distributor to obtain
the latest specifications and before placing your product order.
Copies of documents which have an order number and are referenced in
this document, or other Intel literature, may be obtained by calling
1-800-548-4725, or go to http://www.intel.com/design/literature.htm

Intel processor numbers are not a measure of performance. Processor
numbers differentiate features within each processor family, not
across different processor families. See
http://www.intel.com/products/processor_number for details.

This document contains information on products in the design phase of 
development.

BunnyPeople, Celeron, Celeron Inside, Centrino, Centrino Atom,
Centrino Atom Inside, Centrino Inside, Centrino logo, Core Inside,
FlashFile, i960, InstantIP, Intel, Intel logo, Intel386, Intel486,
IntelDX2, IntelDX4, IntelSX2, Intel Atom, Intel Atom Inside, Intel
Core, Intel Inside, Intel Inside logo, Intel. Leap ahead., Intel. Leap
ahead.  logo, Intel NetBurst, Intel NetMerge, Intel NetStructure,
Intel SingleDriver, Intel SpeedStep, Intel StrataFlash, Intel Viiv,
Intel vPro, XScale, IPLink, Itanium, Itanium Inside, MCS, MMX, Oplus,
OverDrive, Intel PDCharm, Pentium, Pentium Inside, skoool, Sound Mark,
The Journey Inside, VTune, Xeon, and Xeon Inside are trademarks of
Intel Corporation in the U.S. and other countries.


* Other names and brands may be claimed as the property of others.

Copyright (C) 2011, Intel Corporation. All rights reserved.


